   1 "Setup Digitizer"
   2 "Setup Digitizer - Port Settings"
   3 "Setup Digitizer - Select Port"
   4 "Setup Digitizer - Automatic Detection"
   5 "Setup Digitizer - Manual Setup"
   6 "Setup Digitizer - Size, Resolution and Final Check"
   7 "Map Referencing - Coordinate System"
   8 "Locate Fiducial Marks"
   9 "Map Referencing - Digitizer Control Points"
 100 "Are these settings correct"
 101 "Port Settings"
 102 "Scan Resolution:"
 103 "pixel"
 104 "Digitizer Grid Resolution:"
 105 "Digitizer-Grid Unit"
 200 "Received:"
 201 "Number of Received Characters is not constant"
 202 "Press Button %i"
 203 "Trying Automatic Detection"
 204 "Nothing"
 205 "Button"
 206 "None"
 207 "digitizer"
 208 "coordinates"
 209 "diff X"
 210 "diff Y"
 211 "Minimum three points required"
 212 "Scale 1:XXXXXXXXXXXX / XXXXXXXXXXXX"
 213 "Rotation XXXXX.x / XXXXX.x degrees"
 214 "Not enough points"
 215 "Singular Matrix"
 216 "Sigma = %2.1f mm"
 217 "Scale 1:%1.0f / 1:%1.0f"
 218 "Rotation %1.1f / %1.1f degrees"
 219 "Scale 1:%1.0f"
 220 "Rotation %1.1f degrees"
 221 "RowCol (pixels)"
 222 "Photo (mm)"
 223 "diff Row"
 224 "diff Col"
 225 "Grid XY (digitizer grid units)"
 226 "diff Grid X"
 227 "diff Grid Y"
 228 "Specify settings for the selected port:"
 229 "RowCol (sub-pixel precision)"
 230 "Photo (mm in camera-system)"
 300 "BADID: The device identifier is invalid or unsupported"
 301 "BAUDRATE: The device's baud rate is unsupported"
 302 "BYTESIZE: The specified byte size in invalid"
 303 "DEFAULT: The default parameters are in error"
 304 "HARDWARE: The hardware is not available\n(is locked by another device)"
 305 "MEMORY: The function cannot allocate the queues"
 306 "NOPEN: The device is not open"
 307 "OPEN: The device is already open"
 308 "IE error %i"
 309 "Error opening COM port %i\n%S"
 310 "Error opening COM port %i (DCB)"
 311 "Error opening comport %i (State)"
 312 "Digitizer Error"
 313 "WinTab driver not found or not active"
 314 "Error in communication"
 315 "Error"
 316 "No valid fiducial marks found"
 317 "Less than 2 fiducial marks"
 318 "Incorrect positions of fiducial marks"
 319 "Incorrect ordering of 4 fiducial marks"
 320 "Wrong number"
 321 "Too few fiducials, %i needed"
 400 "&Manual"
 401 "&Nr chars"
 402 "&X Pos"
 403 "X &Length"
 404 "&Y Pos"
 405 "Y &Length"
 406 "&Flag pos"
 407 "Flag &Codes"
 408 "&Metric System"
 409 "&Lines per mm"
 410 "&Lines per inch"
 411 "&X-size (mm)"
 412 "&Y-size (mm)"
 413 "&X-size (inch)"
 414 "&Y-size (inch)"
 415 "Digitizer Port:"
 416 "&None"
 417 "COM&1:"
 418 "COM&2:"
 419 "COM&3:"
 420 "COM&4:"
 421 "&Coordinate System"
 422 "Use for Control Points:"
 423 "&Metric (Projected) Coordinates"
 424 "&Geographic Coordinates"
 425 "&Conformal transformation"
 426 "&Affine transformation"
 427 "&WinTab"
 428 "&Baud Rate"
 429 "&Data Bits"
 430 "&Parity"
 431 "&Stop Bits"
 500 "Map Referencing"
 501 "Digitize Point"
 502 "Next Point"
 503 "Delete Point"
