   1 "Calculate minimum and maximum"
   2 "Importing 1.4 raster map '%S'"
   3 "MapMovingAverage"
   4 "MapMovingSurface"
   5 "MapNearestPoint"
   6 "MapTrendSurface"
   7 "MapKriging"
   8 "MapKrigingFromRaster"
   9 "Creating Pyramid layer"
 100 "Calculating minmax of map"
 101 "Init map"
 102 "Creating 3D for map '%S'"
 103 "Calculating"
 104 "Calculating '%S'"
 105 "Create attribute table"
 106 "Write output map"
 107 "Calculate histograms"
 108 "Number of entries in histogram"
 109 "Forward"
 110 "Changes forward %li. Line"
 111 "Backward"
 112 "Changes backward %li. Line"
 113 "Final"
 114 "Determining colors..."
 115 "Create GeoReference"
 116 "Create Domain"
 117 "Create Representation from Look Up Table"
 118 "Scanning forward"
 119 "Scanning backward"
 120 "Interpolate"
 121 "Kriging Error Map of %S"
 122 "Rotating"
 123 "Rasterize"
 124 "Initialize map"
 125 "Resampling map '%S'"
 126 "Converting"
 127 "Scanning input points"
 128 "Finding point pair distances"
 129 "Finding duplicate points  "
 130 "Simple Kriging"
 131 "Ordinary Kriging"
 132 "Anisotropic Kriging"
 133 "Universal Kriging"
 134 "Anisotropic Universal Kriging"
 135 "CoKriging"
 136 "Create Statistics Table column '%S'"
 137 "Cross cluster map and map '%S'"
 138 "Kriging From Raster"
 139 "Converting %S"
 140 "Creating layer %d x %d for map %S"
 141 "stereomate of %S"
 142 "Reading DEM"
 143 "Reading Distance Map"
 144 "Treatment of Flat Area"
 145 "Calculating Flow Direction"
 146 "Calculating Optimized DEM"
 147 "Reading Flow Direction Map"
 148 "Topological Optimization"
 149 "Variable Threshold Computation"
 300 "Calculating Flow Accumulation"
 301 "Writing Flow Accumulation Map"
 302 "Fill single-cell depressions"
 303 "Locate a starting sink"
 304 "Identify outlet cell"
 305 "Fill sinks"
 306 "Flag flat area"
 307 "Calculating Drainage Network Extraction"
 308 "Construct dead-end drainage lines"
 309 "Exterior Drainage Channel Ordering"
 310 "Interior Drainage Channel Ordering"
 311 "Write Drainage Network Raster Map"
 312 "Create Drainage Network Table"
 313 "Create Drainage Network Segment Map"
 314 "Extract Catchment"
 315 "Create catchment raster map"
 316 "Create catchment polygon map"
 317 "Compute catchment attributes"
 318 "Create merged catchment attribute table"
 319 "Calculate the total upstream catchment area"
 320 "Compute the center of polygon"
 321 "Compute the center of drainage channel"
 322 "Merge sub-catchments"
 323 "Calculating overland flow length"
 324 "Reading Flow Accumulation Map"
 325 "Generate Catchment Attributes"
 326 "Extract stream segments"
 327 "Extract stream segment attributes"
 400 "Calculating Land Surface Albedo"
 401 "Atmospheric Effect Correction (SMAC)"
 402 "Compute Land Surface Temperature"
 403 "Compute Surface Emissivity"
 404 "Compute Brightness Temperature"
 405 "Convert raw to radiance/reflectance (MODIS)"
 406 "Surface Energy Balance System (SEBS)"
 407 "Generating SEBS maps..."
 408 "Reference ETo"
 409 "Generating reference ETo map..."
 410 "Converting Radiance Values to Reflectance"
 500 "Find Areas"
 501 "Renumber"
 502 "Created from %S"
 503 "GeoRef of Map %S and GeoRef %S are equal, no resample needed"
 600 "Map export"
 601 "Domain Conversion"
 800 "Invalid file name"
 801 "Cyclic definition"
 802 "Output Object Name already in use"
 803 "Only GeoRef3D allowed in MapApply3D"
 804 "Group factor should be >= 2"
 805 "Invalid row offset: %S"
 806 "Invalid column offset: %S"
 807 "Map too large"
 808 "Invalid domain type for attribute column: '%S'"
 809 "Invalid nr of class: %S"
 810 "2 or more classes needed: %i"
 811 "No more than %i classes allowed: %i"
 812 "Only 1..4 input bands allowed: %i"
 813 "Invalid color type: %S"
 814 "Only picture or domain 'Color' allowed: %S"
 815 "Enlarge factor should be > 1")
 816 "Invalid densify method: '%S'"
 817 "Map is too large. Maximum size is %d lines"
 818 "Same name used for Thiessen Map\nand Distance Map"
 819 "Only value domain allowed for filter %S: %S"
 820 "Invalid filter in MapFilter\n:%S"
 821 "Filter %S\n cannot be applied on map %S"
 822 "Invalid map"
 823 "Incompatible Georefs.\n Pixel size is too different or \n Distance between maps is too large."
 824 "2 or more colors needed: %i"
 825 "Less than 256 colors needed: %i"
 826 "Same name used for error map\nand Kriging Map"
 827 "Invalid rotate method: '%S'"
 828 "Invalid weight function: '%S'\nSyntax: InvDist(exp,limdist) or Linear(exp,limdist)"
 829 "Invalid surface type: '%S'"
 830 "Point size needs to be positive: %i"
 831 "Invalid Resample Method: '%S'"
 832 "Invalid 4th parameter (Patch|NoPatch) '%S'"
 833 "Georef too large"
 834 "Only group domain allowed: '%S'"
 835 "Structure"
 836 "Too many classes for domain %S"
 837 "Map with domain %S can't be exported"
 838 "Unknown error"
 839 "Patching map '%S'"
 840 "Unpatching map '%S'"
 841 "Invalid start row %li"
 842 "Invalid start column %li"
 843 "Invalid row size %li"
 844 "Invalid col size %li"
 845 "Too few valid points (%li), at least %i needed."
 846 "Value Range of map %S too large to export"
 847 "%S cannot interpolate with more than 200 points"
 848 "%S cannot interpolate with more than 25000 points"
 849 "Name of Error Map already used"
 850 "Point map needs to contain at least 2 points"
 851 "Lag Spacing must be greater than 0"
 852 "Lag Spacing may not exceed diagonal size of map"
 853 "Number of Lags must be greater then 0"
 854 "Number of Lags may not exceed 45"
 855 "Number of Lags may not exceed 45"
 856 "Most Lags exceed point map boundaries (due to large lag spacing or too many lags)"
 857 "Minimum number must be at least 1"
 858 "Maximum number may not be less than minimum"
 859 "Limiting distance must be positive and < 2 x greatest point pair distance"
 860 "Degree of trend surface must be 0, 1 or 2"
 861 "Azimuth of Anisotropy must be between -360 and 360 degrees"
 862 "Ratio of Anisotropy must be between 1 and 10"
 863 "Trend degree is 1 so MinNr of points must be 3 or more"
 864 "Trend degree is 2 so MinNr of points must be 6 or more"
 865 "Tolerance must be greater than 0"
 866 "Simple Kriging needs 3 to 6 parameters"
 867 "Ordinary Kriging needs 4 to 9 parameters"
 868 "Anisotropic Kriging needs 5 to 11 parameters"
 869 "Universal Kriging needs 5 to 12 parameters"
 870 "CoKriging needs 7 to 12 parameters"
 871 "Predictand and Covariable Maps don't overlap"
 872 "Illegal Name for Error Map"
 873 "Rasterizing of Attribute Map not possible"
 874 "Kriging From RasterMaps needs 2 to 6 parameters"
 875 "Search radius must be positive"
 876 "Search radius must be large enough, more than 1 pixel"
 877 "Search radius may not exceed 40 pixels"
 878 "Minimum number of input samples is 1"
 879 "Maximum number of input samples is 100"
 880 "Pixel size is not well-defined
 881 "Search-radius Units must be meter(m) or pixels(p)"
 882 "Group factor should not exceed row or column size of input map"
 883 "Map size is illegal (0,0)"
 884 "Missing parameter : %S"
 885 "File %S can not be created"
 886 "The GeoReference should be North oriented."
 887 "Use of attribute maps is not possible: '%S'"
 888 "Source map must have domain class or id"
 889 "Column %S should have value domain"
 890 "Negative probability %.f is not allowed"
 891 "Possible coruption of pyramid layers.\n Pyramid layers will be removed"
 892 "Undefined probability is not allowed"
 893 "Sample set map and table must have the same domain"
 894 "Invalid 5th parameter (GrNoneAllowed|GrNoneDenied) '%S'"
 895 "Use an input map with domain FlowDirection"
 896 "Map should have domain bool"
 897 "Map should have identifier domain"
 898 "Same name used for Longest flow path segment map\nand output Catchment map"
 899 "Error of stream segment map"
 900 "Filter size must be an odd value and greater than 1"
 901 "Invalid number of classes %li"
 902 "Stream order must be greater than 0"
 903 "This fileformat is in its native form nnot supported by ILWIS"
